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ADMISSION NUMBER 	:
CLASS				: 
	
	
	MAXIMUM SCORE
	 ACTUAL
SCORE
	REMARKS

	1
a
b

c

d
	PRESENTATION
Work well pressed ( I ) and folded (1/2 )
Label ( ½  ) firmly fixed (1) without concealing details ( ½ ) and on a single fabric ( ½ )
Pins/needles (½ ) and unnecessary tacking threads (½) and loose threads (½) removed.
Made up for the right half (1). 
	
1 ½ 
2 ½ 

1 ½ 

1


	

	

	
	SUB TOTAL
	6 ½
	
	

	2
a
b

c
d
e
	CUTTING OUT
All seven pieces cut off ( ½ x 7)
C.F of skirt smoothly cut (1) and on straight gain to within 2mm(1)
Smooth cutting of C.B (1) and on grain (1)
C.F of waistband and interfacing smoothly cut ( ½ x 3)
Smooth cutting of skirt lower edge front (1) and back (1)
	
3 ½ 

2
2
1 ½
2
	

	

	
	SUB TOTAL
	11
	
	

	3
a.
b.
c.
d.
e.
f.
g
	DART
Straight stitchery of dart (1) and tapering to nothing ( 1 )
Thread well fastened at the tip.
Correct length of dart (8cm) to within 2mm (7.7-8.3cm)
Correct width of dart (1cm) to within 2mm (0.7-1.3cm)
Dart pressed (1) toward C.B (1)
Correct tension (1)
Dart flat on W.S (1 ) and R.S ( 1)
	
2
1
1
1
2 
1
2

	

	

	
	SUB TOTAL
	10
	
	

	4
a.
b.
c.
d.
e.
f.

g
	PLEATS
Two knife pleats ( ½ x 2) made
Correct depth (2.5cm) 
Pleats pressed towards C.F ( ½ X 2 )
Top stitching straight (½ x2)and close to the edge (½ x2)
Pleats reinforced ( ½ x 2)
Correct length of topstitching 7.5cm (½ x2) to within 3mm (7.2- 7.8cm)
Pleat, well –pressed (1x2) 
	
1
2
1
2
1

1

2



	

	

	
	SUB TOTAL
	10
	
	

	5.
a.

b
c
d.
e

f.
g
h
i


	POCKET
Pocket pieces appropriately placed (1) facing downwards (1)
Pocket pieces attached with straight stitchery (1x2)
Notches matching ( ½ x2) (if trimmed give zero(0)
Smooth stitchery round the pocket bag.
Correct shape (1) and size (1) of pocket (superimpose pattern piece) to within 5mm
Pocket mouth reinforced at base ( ½ ) and top ( ½ )
Understitching (2)
Seam allowance of pocket bag 1.5cm (1)
Pressed towards the front (½)
	

2
2
1
2

2
1
2
1 
½


	

	

	
	SUB TOTAL
	13 ½
	
	

	6

a.

b.
c.

d.
e.
f.

g.

	SIDE SEAM
If not open seam give zero(0)
Seam joined with straight stitchery above (1 ) and below (1) the pocket.
Pocket mouth left unstitched.
Back seam allowance snipped above ( ½ ) and below the pocket ( ½ ) and neatened (1)
Seam well neatened above and below the pocket
Evenness of the neatened seam allowance
Correct size of neatened seam allowance 1cm to within 2mm (0.8-1.2cm)
Seam open (1 )and flat (1 ) at the waistband and at the hem
	

2

1 

2
2
2

2

2





	


	

	
	SUB TOTAL
	13
	
	

	7
a.
b.

c.
d

e

f
g
h
i


j

k
	WAISTBAND
Waistband interfaced (1 ) and correctly done (1 )
Waistband seam joined with straight stitchery (mark by impression) 
Waistband seam evenly trimmed. 
CB of waistband' well snipped  (1 ) and corner pointed ( 1 )
Waistband fixed to skirt with straight stitchery (mark by impression) 
Waistband seam allowance evenly trimmed. 
Waistband well knife edged. 
Straight top stitching of waistband. 
Waistband correctly finished on W.S i.e. well tucked under (1) with neat stitchery (1)If not slip hemming award zero (0).
 Evenness (1) and correct width of the  waistband 2.7cm to within 3mm (2.4 - 3cm) (1).
Loop made on the backwaistband  
Correct positioning (½)
Diameter of the loop 1.3 cm (½)
Loop reinforced along the whole length (1)

	
2

2
1

2

2
1
1
2

2


2

½
½
1
	

	

	
	SUB TOTAL
	19
	
	

	
a
b
c
d
	PREPARATION OF THE SKIRT HEM AND EVEN TACKINg
Hem edgestitched  (1) and folded(1)
Even in width(2)
Hem made on the W.S (1)
 Even tacking made (1)and even (1)

	
2
2
1
2


	
	

	
	Sub total
	7
	
	

	
	TOTAL
	90
	
	

	
	FINAL MARK =   ACTUAL SCORE
                                                                                    2
	45
	
	




