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GRADE 10 – BUILDING CONTRUCTION    
Time: 2 Hours
LEARNER’S DETAILS
Name: _____________________________________________________________.  School: ____________________________________________.
Assessment Number: _______________________________________________.      Date: ____________________________________________.
School Code: ______________________________________________________.        Signature: _______________________________________.
INSTRUCTIONS TO CANDIDATES
1. Write your name in the spaces provided above.
2. Write the name of your school and your stream in the spaces provided.
3. Write your admission number and the date of the assessment in the spaces provided.
4. This paper consists of two sections: A and B.
5. Answer all questions in section A and section B.
6. Answer the questions in English.
7. All answers MUST be written in the spaces provided in the paper.
8. Do NOT remove any page from this question paper.
FOR OFFICIAL USE ONLY (EXAMINER’S USE)
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SECTION A (30 MARKS)
[image: ][image: ]                                                                                   Answer ALL questions in this section.                                                                                                                                                                                  1. Study the samples represented below and answer the questions. 
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               A                              B                             C


      a) Identify the building materials represented by A, B and C. (3 marks)
A. ......................................................................................
B. ......................................................................................
C. ......................................................................................
b) State one use of material A in building construction. (1 mark)
...................................................................................................................................................................................
c) State one property of a good building stone. (1 mark)
......................................................................................................................................................................................
2. Study the simplified cross-section below.
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a) Identify the component labelled X.   (1 mark)
..............................................................................................
b) State two functions of  X.   (2 marks)
i. .................................................................................................................................................................................
ii. ................................................................................................................................................................................
c) State two factors that influence foundation depth.   (2 marks)
i. ..........................................................................................................................................................................................
ii. ........................................................................................................................................................................................


3. Study the tools shown below.
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a) Identify any two setting-out tools represented above. (2 marks)
A. ......................................................................................
B. ...................................................................................
b) State one use of a builder's square. (1 mark)
...................................................................................................................................................................................
4. Study the line below.
A ●────────────────────────────● B
            600 mm
The line represents a wall on a building drawing. The actual wall is 6 metres long.
a) Calculate the scale of the drawing. (2 marks)



b) State one importance of scale in building drawing. (1 mark)
...........................................................................................................................................................................................................................................................................................................................................................................................

5. Study the simplified building representation.
             FRONT ELEVATION

             ┌─────────────┐
             │  ┌───────┐  │
             │  │       │  │
             │  │       │  │
             │  └───────┘  │
             │     ┌──┐    │
             │     │  │    │
             └─────┴──┴────┘
a) Identify the type of building drawing shown.   (1 mark)
..............................................................................................
b) State two pieces of information that may be obtained from this type of drawing. (2 marks)
i. ............................................................................................
ii. ...........................................................................................
6. Susan was asked to list the materials used in making concrete.
      
   a) Identify the four basic materials. (4 marks)
A. ......................................................................................
B. ......................................................................................
C. ......................................................................................
D. ......................................................................................
b) State one purpose of water in concrete. (1 mark)
...........................................................................................................................................................................................................................................................................................................................................................................................
[image: ]7. Study the excavation shown below.







a) Identify the construction activity represented by the diagram. (1 mark)
...............................................................................................................................................................
b) Name one danger associated with unsupported deep excavations.(1 mark)
.......................................................................................................................................................................................
c) State one method of preventing collapse of the excavation sides.(1 mark)
...................................................................................................................................................................................
8. Study the diagram below.
[image: ]
a) Identify the construction support represented by the shaded members. .

...........................................................................................................................................
b) State two reasons for providing this support. (2 marks)
i. ..................................................................................................................................................................................
ii. ...................................................................................................................................................................................
[image: ]9. Study the simplified floor construction.



T



a) Identify the layer represented by the T. (1 mark)
..............................................................................................

b) State one purpose of hardcore in floor construction. (1 mark)
..............................................................................................
c) State one reason for compacting the ground before laying a floor. (1 mark)
...................................................................................................................................................................................
10. Study the pipe fittings below.
           A                                B                                  C
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a) Identify fittings A, B and C. (3 marks)
A. ......................................................................................
B. ......................................................................................
C. ......................................................................................
b) State one function of a tee fitting. (1 mark) 
.........................................................................................................................................................................................
c) Name one material used for manufacturing water pipes. (1 mark)
.................................................................................................................................................................................
SECTION B: 50 MARKS
Answer ALL questions.
11. A contractor has been given a piece of land on which a residential building is to be constructed. The site contains bushes, tree stumps, loose soil and some stones.
a)Identify four activities that should be undertaken during site preparation.(4 marks)
i. ......................................................................................................................................................................... 
ii. .........................................................................................................................................................................  
iii. .........................................................................................................................................................................  
iv. .......................................................................................................................................................................... 

b)Explain three factors that should be investigated before construction begins.(3 marks)
i. ......................................................................................................................................................................... 
ii. .........................................................................................................................................................................  
iii. .........................................................................................................................................................................  
c) State three reasons why setting out must be accurate. (3 marks)
i. ......................................................................................................................................................................... 
ii. .........................................................................................................................................................................  
iii. .........................................................................................................................................................................  
12. Study the setting-out illustration below.
        A────────────────────────B
        │                        │
        │                        │
        │                        │
        │                        │
        D────────────────────────C

        AB = DC
        AD = BC
a)
Identify the shape of the building being set out. (1 mark)
..............................................................................................
b) Explain four steps involved in setting out the building shown above. (4 marks)
i. ......................................................................................................................................................................... 
ii. .........................................................................................................................................................................  
iii. .........................................................................................................................................................................  
iv. .......................................................................................................................................................................... 
c) State three methods/tools that can be used to ensure that corners A, B, C and D are accurately positioned.
(3 marks)
i. ......................................................................................................................................................................... 
ii. .........................................................................................................................................................................  
iii. .........................................................................................................................................................................  
d) State two checks that should be made before excavation begins. (2 marks)
i. ............................................................................................................................................................................
ii. ..........................................................................................................................................................................
13. Study the simplified plan below.
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a) Identify the type of drawing shown. (1 mark)
..............................................................................................
b) Name four features visible on the drawing. (4 marks)
i. ......................................................................................................................................................................... 
ii. .........................................................................................................................................................................  
iii. .........................................................................................................................................................................  
iv. .......................................................................................................................................................................... 
c) The actual length of the building is 8 metres. On a drawing it measures 16 cm.
Calculate the scale. (3 marks)


d) State two reasons why dimensions are included on building drawings. (2 marks)
i. ..............................................................................................................................................................................
ii. ..............................................................................................................................................................................
 14. 
a) Identify four components shown in the cross-section. (4 marks)
i. ............................................................................................
ii. ...........................................................................................
iii. ..........................................................................................
iv. ..........................................................................................
b) Explain three functions of the foundation. (3 marks)
i. ..........................................................................................................................................................................................
ii. .........................................................................................................................................................................................
iii. ........................................................................................................................................................................................
c)State three requirements of a good ground floor.(3 marks)
i. .........................................................................................................................................................................................
ii. ......................................................................................................................................................................................
iii. ......................................................................................................................................................................................
15.Study the two illustrations below.
A. CONCRETE MIXING
             WATER
               ↓
       ┌───────────────┐
       │   CEMENT      │
       │ + SAND        │
       │ + AGGREGATE   │
       └───────────────┘
              ↓
           MIXING
              ↓
           CONCRETE
B. PLUMBING SYSTEM
       WATER TANK
          │
          │
          ▼
      ┌─────────┐
      │  VALVE  │
      └────┬────┘
           │
           ├───────────┐
           │           │
           ▼           ▼
         TAP          TAP
a)
From illustration A, state four operations involved in producing good concrete. (4 marks)
i. ............................................................................................
ii. ...........................................................................................
iii. ..........................................................................................
iv. ..........................................................................................
b)
State three functions of a valve in a water-supply system. (3 marks)
i. ............................................................................................
ii. ...........................................................................................
iii. ..........................................................................................
c)
State three safety precautions when carrying out plumbing work.
(3 marks)
i. ............................................................................................
ii. ...........................................................................................
iii. ..........................................................................................









GRADE 10 – BUILDING CONSTRUCTION
MARKING SCHEME
1. 
a) Identify the materials:
A. Stone – 1 mark
B. Brick – 1 mark
C. Aggregate/ballast – 1 mark
b) One use of stone:
· Construction of walls. 
· Construction of foundations. 
· Construction of retaining walls. 
· Road works. 
Any one – 1 mark
c) One property of good building stone:
· Strong. 
· Durable. 
· Hard. 
· Resistant to weathering. 
· Free from cracks. 
· Has good appearance. 
Any one – 1 mark
2. 
a) The component identified as FOOTING is the foundation footing/base.
1 mark
b) Two functions of a foundation/footing:
· Transfers building loads safely to the ground. 
· Distributes the load over a larger area of soil. 
· Provides a stable base for the building. 
· Prevents excessive settlement. 
Any 2 × 1 = 2 marks
c) Two factors influencing foundation depth:
· Type and bearing capacity of soil. 
· Load/weight of the building. 
· Depth of firm bearing stratum. 
· Groundwater conditions. 
· Nature of the site. 
Any 2 × 1 = 2 marks
3. 
a) Identification:
The intended setting-out tools are:
A. Ranging rod – 1 mark
B. Builder's square – 1 mark
Accept another correctly identified setting-out tool where the learner's identification matches the intended illustration.
b) Use of a builder's square:
· To set out/check a right angle of 90°. 
· To ensure corners of a building are square. 
1 mark
Total: 3 marks
4. 
Actual length = 6 m = 600 cm
Drawing length = 600 mm = 60 cm
Therefore:
Scale=60600\text{Scale}=\frac{60}{600} =110=\frac{1}{10} 
Scale = 1:10
2 marks
Note: The original question illustration states 600 mm while the text states 6 metres. Therefore, the correct interpretation is that the drawing line is 600 mm, giving a scale of 1:10.
b) Importance of scale:
· Allows large objects/buildings to be represented on a manageable drawing sheet. 
· Maintains proportional accuracy. 
· Enables actual dimensions to be determined from the drawing. 
Any 1 – 1 mark
5. 
a) The drawing is a front elevation.
1 mark
b) Information obtained from an elevation:
· External appearance of the building. 
· Position and size of doors. 
· Position and size of windows. 
· Height of the building. 
· Roof shape. 
· Vertical dimensions. 
· External finishes. 
Any 2 × 1 = 2 marks
6. 
a) Identification of the four basic materials:
A. Cement – 1 mark
B. Sand/fine aggregate – 1 mark
C. Coarse aggregate/ballast – 1 mark
D. Water – 1 mark
b) Purpose of water:
· It reacts with cement during hydration. 
· It makes the mixture workable. 
· It assists in bonding the ingredients. 
Any one – 1 mark
7. 
a) Excavation of a foundation trench.
1 mark
b) One danger:
· Collapse of trench sides. 
· Burial of workers. 
· Injury or death. 
· Falling materials into the excavation. 
Any one – 1 mark
c) One method of preventing collapse:
· Timbering/shoring. 
· Proper battering/sloping of sides. 
· Providing suitable excavation support. 
Any one – 1 mark
8. 
a) The support is timbering/shoring of an excavation.
1 mark
b) Two reasons for timbering:
· Prevents collapse of excavation sides. 
· Protects workers from being buried or injured. 
· Maintains the shape and dimensions of the trench. 
· Improves safety during excavation. 
Any 2 × 1 = 2 marks
Total: 3 marks
9. 
a) The shaded layer is hardcore.
1 mark
b) One purpose of hardcore:
· Provides a firm and stable base for the floor slab. 
· Helps raise the floor level. 
· Improves drainage and reduces settlement when properly selected and compacted. 
Any one – 1 mark
c) Reason for compacting ground:
· To reduce settlement. 
· To provide a firm and stable base. 
· To increase the bearing capacity of the ground. 
Any one – 1 mark
10. 
a) Identification:
A. Elbow– 1 mark
B. Union – 1 mark
C. Cross  – 1 mark
b) Function of a tee:
· Provides a branch connection from the main pipe. 
· Divides/directs water into another pipe. 
1 mark
c) One material used for water pipes:
· PVC/uPVC. 
· Copper. 
· PEX. 
· Galvanised steel. 
Any one – 1 mark
11. 
a) Four site-preparation activities
1. Clearing vegetation – removing bushes, grass and unwanted trees. 
2. Removing tree stumps and roots – clearing obstacles that may interfere with construction. 
3. Removing stones and debris – preparing a clean construction area. 
4. Demolition/removal of unwanted structures where applicable. 
5. Levelling/grading the site. 
6. Disposal of waste to an appropriate location. 
Any 4 × 1 = 4 marks
b) Three factors to investigate before construction
1. Soil condition – determine the type and bearing capacity of soil. 
2. Site levels/topography – establish slopes and levels of the land. 
3. Drainage/groundwater – determine water conditions and drainage requirements. 
4. Access – determine how workers, materials and equipment will reach the site. 
5. Availability of services – establish water, electricity and other services. 
6. Boundaries – establish the correct site boundaries. 
Any 3 × 1 = 3 marks
c) Three reasons for accurate setting out
· Ensures the building is positioned correctly on the site. 
· Ensures correct building dimensions. 
· Ensures walls are correctly aligned. 
· Ensures corners are accurately positioned. 
· Prevents costly construction errors. 
· Ensures the building follows the approved drawings. 
Any 3 × 1 = 3 marks
Question 11 = 10 marks
12. 
a)
The shape is a rectangle/rectangular building.
1 mark
b) Four steps in setting out
A suitable procedure is:
1. Study the building plan and establish the required dimensions. 
2. Establish a baseline from which the building will be measured. 
3. Fix pegs at the required positions. 
4. Stretch string lines between the pegs to indicate wall positions. 
5. Establish right angles using a builder's square or 3:4:5 method. 
6. Measure the required length and width. 
7. Check the diagonals to ensure the corners are correctly positioned. 
8. Fix profile boards outside the excavation area. 
Any 4 × 1 = 4 marks
c) Three methods/tools for accurate positioning
· Builder's square. 
· Tape measure. 
· 3:4:5 method. 
· Theodolite. 
· Ranging rods. 
· Spirit level. 
· Optical/laser level. 
· Checking diagonals. 
Any 3 × 1 = 3 marks
d) Two checks before excavation
· Check the building dimensions against the working drawing. 
· Check that corners are square/right-angled. 
· Check the diagonals. 
· Check alignment and levels. 
· Confirm the building is correctly positioned within the site boundaries. 
Any 2 × 1 = 2 marks
Question 12 = 10 marks
13.
a)
The drawing is a building plan/floor plan.
1 mark
b) Four features visible
Any four:
· Bedrooms. 
· Living room. 
· Kitchen. 
· Internal walls. 
· External walls. 
· Room divisions. 
· Dimensions. 
· Door/window positions. 
Any 4 × 1 = 4 marks
c) Scale calculation
Actual length = 8 metres
Convert to centimetres:
8m=800cm8m = 800cm 
Drawing length = 16 cm
Scale=16800\text{Scale}=\frac{16}{800} =150=\frac{1}{50} 
Scale = 1:50
Working – 2 marks
Answer – 1 mark
d) Two reasons for including dimensions
· To indicate the actual size of building components. 
· To guide the construction team during construction. 
· To enable accurate setting out. 
· To reduce construction errors. 
· To indicate distances between different building elements. 
Any 2 × 1 = 2 marks
Question 13 = 10 marks
14. 
a) Four components shown
Any four:
i. Wall – 1 mark
ii. Foundation wall – 1 mark
iii. Footing – 1 mark
iv. Hardcore – 1 mark
v. Compacted ground – 1 mark
Any 4 = 4 marks
b) Three functions of a foundation
· Transfers the load of the building safely to the ground. 
· Distributes the building load over a suitable area. 
· Provides stability to the building. 
· Reduces excessive settlement. 
· Prevents movement caused by unstable ground. 
Any 3 × 1 = 3 marks
c) Three requirements of a good ground floor
· It should be strong enough to carry imposed loads. 
· It should be level and even. 
· It should be durable. 
· It should resist ground moisture. 
· It should be properly compacted and supported. 
· It should have an appropriate finish. 
· It should provide suitable thermal insulation where required. 
Any 3 × 1 = 3 marks
Question 14 = 10 marks
15. 
a) Four operations involved in producing good concrete
1. Batching/measuring the ingredients in the required proportions. 
2. Mixing cement, sand and aggregate thoroughly. 
3. Adding water in the correct quantity. 
4. Placing the concrete in the required position. 
5. Compacting the concrete to remove trapped air. 
6. Finishing the surface. 
7. Curing the concrete adequately. 
Any 4 × 1 = 4 marks
b) Three functions of a valve
· Controls the flow of water. 
· Stops the flow of water when necessary. 
· Allows sections of the plumbing system to be isolated for maintenance or repair. 
· Regulates water flow in suitable applications. 
Any 3 × 1 = 3 marks
c) Three plumbing safety precautions
· Wear appropriate PPE such as gloves and safety footwear. 
· Use the correct tools for each task. 
· Turn off the water supply before repairing or modifying pipes. 
· Keep the working area clean and free from hazards. 
· Handle sharp tools carefully. 
· Ensure electrical equipment is kept away from water. 
· Inspect tools before use. 
Any 3 × 1 = 3 marks
















KENYA CERTIFICATE OF BASIC EDUCATION
SENIOR SCHOOL ASSESSMENT
TERM 3: PROJECT BASED ASSESSMENT 2026
GRADE 10 – BUILDING CONTRUCTION    
Time: 2 Hours
LEARNER’S DETAILS
Name: _____________________________________________________________.  School: ____________________________________________.
Assessment Number: _______________________________________________.      Date: ____________________________________________.
School Code: ______________________________________________________.        Signature: _______________________________________.
PROJECT-BASED ASSESSMENT TEST
PROJECT BRIEF
You have been asked to design and construct a simple masonry structure suitable for a small domestic building.
The project should demonstrate your ability to:
· Interpret a building requirement. 
· Prepare a simple floor plan. 
· Produce a basic building drawing. 
· Select appropriate materials and tools. 
· Set out the structure. 
· Construct a masonry wall section. 
· Observe safety requirements. 
· Evaluate the completed project. 
The teacher will provide or approve the available materials before construction begins.
SECTION A: PROJECT DESIGN AND FLOOR PLAN – 6 MARKS
1. Prepare a simple floor plan of a small building containing:
· One main room 
· One additional room 
· A door 
· At least two windows 
· Internal dimensions 
· External dimensions 
(4 marks)



Space for floor plan:



































2. Label the following on your floor plan:
a) Door – ½ mark
b) Windows – ½ mark
c) Rooms – ½ mark
d) Dimensions – ½ mark
Total: 2 marks
Drawing requirements
The learner should demonstrate:
· Use of appropriate drawing instruments. 
· Reasonable proportion and neatness. 
· Correct use of conventional building symbols. 
· Clear labelling and dimensions. 
SECTION B: PROJECT PLANNING – 3 MARKS
3. List THREE materials required for the construction project.(1½ marks)
i. ....................................................................................
ii. ...................................................................................
iii. ..................................................................................
4. List THREE tools/equipment required for the project.(1½ marks)
i. ....................................................................................
ii. ...................................................................................
iii. ..................................................................................
SECTION C: PRACTICAL CONSTRUCTION – 8 MARKS
Using your approved plan, construct a small section of the proposed masonry wall.
The wall section should demonstrate appropriate:
	Assessment Indicator
	Marks

	Setting out according to the plan
	1

	Correct selection and preparation of materials
	1

	Preparation and appropriate use of mortar
	1

	Correct laying of bricks/blocks
	2

	Maintaining line, level and verticality
	1

	Correct bonding
	1

	Neatness and quality of workmanship
	1

	TOTAL
	8


SECTION D: SAFETY AND WORKSITE MANAGEMENT – 2 MARKS
5. Demonstrate the following during the project:
a) Safe and correct use of tools and equipment – 1 mark
b) Proper organisation and cleanliness of the work area – 1 mark
SECTION E: PROJECT EVALUATION – 1 MARK
6. State ONE challenge experienced during the project and explain how you addressed it.(1 mark)
Challenge:
............................................................................................................................................................................................................................................................................................................................................................................................
How it was addressed:
...........................................................................................................................................................................................................................................................................................................................................................................................

PROJECT ASSESSMENT RUBRIC
	Competency Area
	Exceeds Expectations
	Meets Expectations
	Approaching Expectations
	Below Expectations

	Floor plan/drawing
	Accurate, neat, correctly dimensioned and well labelled
	Generally accurate with minor errors
	Several errors in symbols/dimensions
	Incomplete or poorly presented

	Planning
	Materials and tools selected appropriately
	Most requirements identified
	Some requirements identified
	Poor planning

	Construction
	Excellent workmanship, alignment and bonding
	Good workmanship with minor errors
	Some construction errors
	Major errors/incomplete work

	Safety
	Consistently demonstrates safe practices
	Generally safe
	Requires occasional reminders
	Frequently ignores safety requirements

	Evaluation
	Clearly identifies problem and solution
	Identifies problem and solution
	Limited explanation
	Unable to evaluate project


TEACHER'S PROJECT RECORD
Learner's Name: __________________________________________
Grade: 10 ____________
Admission No.: __________________
Date: __________________
	No.
	Assessment Area
	Max. Marks
	Score

	1
	Floor plan and building drawing
	6
	

	2
	Project planning
	3
	

	3
	Practical construction
	8
	

	4
	Safety and worksite management
	2
	

	5
	Project evaluation
	1
	

	
	TOTAL
	20
	


Teacher's Observation:
..............................................................................................................
..............................................................................................................
Teacher's Name: __________________________________________
Signature: ______________________
Date: __________________________





GRADE 10 BUILDING TECHNOLOGY
PROJECT-BASED ASSESSMENT – MARKING SCHEME
Project: Design and Construction of a Simple Masonry Structure
Total Marks: 20
SECTION A: DRAWING AND FLOOR PLAN – 6 MARKS
1. Floor Plan – 4 Marks
Award marks as follows:
	Requirement
	Marks

	Correct overall layout/proportion of the building
	1

	Correct representation of walls and room arrangement
	1

	Appropriate door and window positions/symbols
	1

	Neatness and use of appropriate drawing conventions
	1

	Total
	4


2. Labelling and Dimensioning – 2 Marks
	Requirement
	Marks

	Rooms clearly labelled
	½

	Door correctly indicated/labelled
	½

	Windows correctly indicated/labelled
	½

	Internal/external dimensions shown appropriately
	½

	Total
	2


Section A Total = 6 Marks
SECTION B: PROJECT PLANNING – 3 MARKS
3. Materials – 1½ Marks
Award ½ mark for each correct material, up to 3 materials.
Accept:
· Bricks/blocks 
· Cement 
· Sand 
· Water 
· Damp-proof materials 
· Timber where applicable 
· Other appropriate building materials 
Maximum = 1½ marks
4. Tools/Equipment – 1½ Marks
Award ½ mark for each correct tool/equipment, up to 3.
Accept:
· Brick trowel 
· Spirit level 
· Tape measure 
· Plumb bob 
· Builder's line 
· Mason's square 
· Shovel 
· Bucket 
· Straight edge 
· Other appropriate tools 
Maximum = 1½ marks
Section B Total = 3 Marks
SECTION C: PRACTICAL CONSTRUCTION – 8 MARKS
	Assessment Indicator
	Marking Points
	Marks

	Setting out
	Correctly transfers dimensions/layout from the plan to the work area
	1

	Material selection/preparation
	Selects and handles suitable materials correctly
	1

	Mortar preparation/use
	Prepares/uses mortar appropriately and consistently
	1

	Laying bricks/blocks
	Correct positioning and laying of units
	2

	Line, level & verticality
	Maintains straightness, level and plumb
	1

	Bonding
	Applies an appropriate masonry bond correctly
	1

	Workmanship/neatness
	Joints, corners and finished work are neat
	1

	TOTAL
	
	8


Detailed Awarding Guidance
Setting out – 1 mark
· Correct measurements and positions – ½ 
· Correct use of line/square or other setting-out method – ½ 
Material selection/preparation – 1 mark
· Correct materials selected – ½ 
· Materials properly prepared/handled – ½ 
Mortar – 1 mark
· Appropriate mixing/preparation – ½ 
· Appropriate application – ½ 
Laying bricks/blocks – 2 marks
· Correct positioning – 1 
· Proper and consistent laying – 1 
Line, level and verticality – 1 mark
· Maintains horizontal alignment – ½ 
· Maintains verticality/plumb – ½ 
Bonding – 1 mark
· Correct bond selected – ½ 
· Bond correctly maintained – ½ 
Workmanship – 1 mark
· Neat joints/finish – ½ 
· Overall quality of construction – ½ 
SECTION D: SAFETY AND WORKSITE MANAGEMENT – 2 MARKS
5. Safety Practices
	Requirement
	Marks

	Uses tools and equipment safely and correctly
	1

	Maintains a clean, organised and safe working area
	1

	Total
	2


Award only when the learner actually demonstrates the practice during the project.
SECTION E: PROJECT EVALUATION – 1 MARK
6. Challenge and Solution
Award:
· Correctly identifies a realistic challenge – ½ mark 
· Gives an appropriate way of addressing the challenge – ½ mark 
Total = 1 mark
Examples of acceptable challenges:
· Shortage of materials 
· Difficulty maintaining alignment 
· Incorrect mortar consistency 
· Limited working space 
· Difficulty maintaining dimensions 
PERFORMANCE LEVEL
	Score
	Performance

	17–20
	Exceeds Expectations

	13–16
	Meets Expectations

	9–12
	Approaching Expectations

	0–8
	Below Expectations


Teacher's Overall Comment:
.............................................................................................................................................................................................................................................................................................................................................................................................
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